<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="3" x2="3" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3" y1="0" x2="47" y2="0" width="0" layer="20"/>
<wire x1="47" y1="0" x2="62" y2="0" width="0" layer="20"/>
<wire x1="62" y1="0" x2="65" y2="3" width="0" layer="20" curve="90"/>
<wire x1="65" y1="3" x2="65" y2="97" width="0" layer="20"/>
<wire x1="65" y1="97" x2="62" y2="100" width="0" layer="20" curve="90"/>
<wire x1="62" y1="100" x2="3" y2="100" width="0" layer="20"/>
<wire x1="3" y1="100" x2="0" y2="97" width="0" layer="20" curve="90"/>
<wire x1="0" y1="97" x2="0" y2="37.5" width="0" layer="20"/>
<hole x="3.5" y="3.5" drill="2.8"/>
<hole x="3.5" y="52.5" drill="2.8"/>
<hole x="61.5" y="52.5" drill="2.8"/>
<hole x="61.5" y="3.5" drill="2.8"/>
<wire x1="0" y1="18.5" x2="0" y2="3" width="0" layer="20"/>
<text>GND</text>
<text>Vio</text>
<text>BMB2</text>
<text>BMB1</text>
<text>BMA1</text>
<text>BMA2</text>
<text>GND</text>
<text>Vm</text>
<text>EN</text>
<text>SDI/CFG1</text>
<text>SCK/CFG2</text>
<text>CSN/CFG3</text>
<text>SDO/CFG0</text>
<text>DCO</text>
<text>Step</text>
<text>Dir</text>
<text>DIAG0</text>
<text>DIAG1</text>
<text>GND</text>
<text>Vio</text>
<text>BMB2</text>
<text>BMB1</text>
<text>BMA1</text>
<text>BMA2</text>
<text>GND</text>
<text>Vm</text>
<text>EN</text>
<text>SDI/CFG1</text>
<text>SCK/CFG2</text>
<text>CSN/CFG3</text>
<text>SDO/CFG0</text>
<text>DCO</text>
<text>Step</text>
<text>Dir</text>
<text>DIAG0</text>
<text>DIAG1</text>
<circle x="24" y="27" radius="18" width="0.001" layer="20"/>
<wire x1="45" y1="19" x2="45" y2="4" width="2" layer="20"/>
<wire x1="45" y1="19" x2="45" y2="4" width="2" layer="46"/>
<wire x1="1" y1="19.5" x2="3" y2="19.5" width="0.001" layer="20"/>
<wire x1="3" y1="19.5" x2="4" y2="20.5" width="0.001" layer="20" curve="90"/>
<wire x1="4" y1="20.5" x2="4" y2="35.5" width="0.001" layer="20"/>
<wire x1="4" y1="35.5" x2="3" y2="36.5" width="0.001" layer="20" curve="90"/>
<wire x1="3" y1="36.5" x2="1" y2="36.5" width="0.001" layer="20"/>
<wire x1="1" y1="36.5" x2="0" y2="37.5" width="0.001" layer="20" curve="-90"/>
<wire x1="0" y1="18.5" x2="1" y2="19.5" width="0.001" layer="20" curve="-90"/>
<hole x="61.5" y="96.5" drill="2.8"/>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>GND</text>
<text>5V</text>
<text>RPM</text>
<text>PWM</text>
<text>GND</text>
<text>3V3</text>
<text>SCL</text>
<text>SDA</text>
<text>Planktoscope
HAT</text>
<text>designed by
Romain BAZILE
</text>
<text>for PlanktonPlanet</text>
<text>v0.1 - beta
2021-02-01</text>
<text>TMC5160
SilentStepStick</text>
<text>TMC5160
SilentStepStick</text>
</plain>
<libraries>
<library name="FLYFISH">
<packages>
<package name="SOIC8">
</package>
</packages>
</library>
<library name="pinhead-2">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de, Modified by Cougar@CasaDelGato.Com&lt;/author&gt;</description>
<packages>
<package name="1X08-S">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 2.54</description>
</package>
</packages>
</library>
<library name="we-con">
<description>Connectors, Sockets...</description>
<packages>
<package name="MA02-1">
</package>
</packages>
</library>
<library name="SparkFun-IC-Power">
<description>&lt;h3&gt;SparkFun Power Driver and Management ICs&lt;/h3&gt;
In this library you'll find anything that has to do with power delivery, or making power supplies.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;LDOs&lt;/li&gt;
&lt;li&gt;Boost/Buck controllers&lt;/li&gt;
&lt;li&gt;Charge pump controllers&lt;/li&gt;
&lt;li&gt;Power sequencers&lt;/li&gt;
&lt;li&gt;Power switches&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="PScope">
<packages>
<package name="SO-8EP_DIO">
</package>
<package name="POWERDI3333-8_UX_DIO">
</package>
<package name="CONN_S4B-XH-SM4-TB_JST">
</package>
<package name="40MM_FAN">
</package>
<package name="DBV6">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
<library name="Capacitor">
<description>&lt;B&gt;Capacitors - Fixed, Variable, Trimmers</description>
<packages>
<package name="CAPMP6032X280N">
<description>Molded Body, 6.00 X 3.20 X 2.80 mm body
&lt;p&gt;Molded Body package with body size 6.00 X 3.20 X 2.80 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="TESTPOINT_PAD_2MM">
<description>Testpoint - Pad</description>
</package>
<package name="_0805MP">
<description>&lt;b&gt;0805 MicroPitch&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_3_1-NC_PASTE_SILK">
</package>
<package name="SMT-JUMPER_2_NO_SILK">
</package>
</packages>
</library>
<library name="SparkFun-Coils">
<description>&lt;h3&gt;SparkFun Coils&lt;/h3&gt;
In this library you'll find magnetics.

&lt;p&gt;&lt;b&gt;SparkFun Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;Inductors&lt;/li&gt;
&lt;li&gt;Ferrite Beads&lt;/li&gt;
&lt;li&gt;Transformers&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;

&lt;br&gt;
&lt;p&gt;We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.&lt;/p&gt;</description>
<packages>
<package name="SRN6045">
<description>&lt;h3&gt;SRN6045 series  footprint&lt;/h3&gt;
&lt;p&gt;Roughly based on the recommendation in this &lt;a href="http://www.mouser.com/ds/2/54/RN6045-778135.pdf"&gt;datasheet&lt;/a&gt;.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
<package name="SOT26">
<description>Footprint for SOT-26 part DMP2240UDM</description>
</package>
</packages>
</library>
<library name="Diode">
<description>&lt;B&gt;PN Junction, BridgeRectifier, Zener, Schottky, Switching</description>
<packages>
<package name="DIOM5226X290N">
<description>Molded Body, 5.20 X 2.60 X 2.90 mm body
&lt;p&gt;Molded Body package with body size 5.20 X 2.60 X 2.90 mm&lt;/p&gt;</description>
</package>
<package name="SODFL1608X70">
<description>SODFL, 1.60 mm span, 1.20 X 0.80 X 0.70 mm body
&lt;p&gt;SODFL package with 1.60 mm span with body size 1.20 X 0.80 X 0.70 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Connector">
<description>&lt;b&gt;Pin Headers,Terminal blocks, D-Sub, Backplane, FFC/FPC, Socket</description>
<packages>
<package name="2X20">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="OPL_Connector">
<description>&lt;b&gt;Seeed Open Parts Library (OPL) for the Seeed Fusion PCB Assembly Service&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
This library is designed for use with parts that are stocked by Seeed and can be used directly with Seeed's turnkey PCB assembly service. By using only parts in the OPLs, the PCBA production time can be drastically reduced.

&lt;br&gt;&lt;br&gt;
We continuously work to make sure these libaries are accurate and up to date. Make sure you update to the latest version via the Library Manager. We will not take responsibility for the use of out-of-date libraries.

&lt;br&gt;&lt;br&gt;
If you discover any discreprancies or would like to contribute, please &lt;b&gt;&lt;a href="mailto:fusion@seeed.cc?Subject=Regarding the Seeed OPL..." target="_top"&gt;get in touch&lt;/a&gt;&lt;/b&gt; or fork the &lt;b&gt;&lt;a href="https://github.com/Seeed-Studio/OPL_Eagle_Library" title="Seeed OPL Eagle GitHub Repository"&gt;GitHub&lt;/a&gt;&lt;/b&gt; repository. 
&lt;br&gt;&lt;br&gt;

&lt;b&gt;&lt;a href="https://www.seeedstudio.com/opl.html" title="https://www.seeedstudio.com/opl.html"&gt;Seeed Fusion PCBA OPL&lt;/a&gt;
&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/prototype-pcb-assembly.html" title="Seeed Fusion PCB Assembly Service"&gt;Seeed Fusion PCB Assembly Service&lt;/a&gt;
&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/fusion_pcb.html"&gt;Order PCB/PCBA Now&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;
&lt;a href="https://www.seeedstudio.com"&gt;www.seeedstudio.com&lt;/a&gt;</description>
<packages>
<package name="H4-2.54">
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RV-3028">
<description>Footprint for the RV-3028 I&lt;sup&gt;2&lt;/sup&gt;C RTC</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Wurth_Elektronik_Passive_Capacitors_rev19a">
<description>&lt;BR&gt;Wurth Elektronik - Electrolytic Capacitors,Ceramic Capacitors &amp; Film Capacitors&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;

Eagle Version 6, Library Revision 2019a, 2019-08-07&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="8X3.5X0.9(DXAXB)">
</package>
</packages>
</library>
<library name="OPL_Discrete_Semiconductor">
<description>&lt;b&gt;Seeed Open Parts Library (OPL) for the Seeed Fusion PCB Assembly Service
&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/opl.html" title="https://www.seeedstudio.com/opl.html"&gt;Seeed Fusion PCBA OPL&lt;/a&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com/fusion_pcb.html"&gt;Order PCB/PCBA&lt;/a&gt;&lt;br&gt;&lt;br&gt;
&lt;a href="https://www.seeedstudio.com"&gt;www.seeedstudio.com&lt;/a&gt;
&lt;br&gt;&lt;/b&gt;</description>
<packages>
<package name="SOD-123">
<description>&lt;b&gt;Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Inductor">
<description>&lt;B&gt;Inductors - Fixed, Variable, Coupled</description>
<packages>
<package name="INDM3225X240">
<description>Molded Body, 3.20 X 2.50 X 2.40 mm body
&lt;p&gt;Molded Body package with body size 3.20 X 2.50 X 2.40 mm&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-4">
<description>&lt;h3&gt;Screw Terminal  3.5mm Pitch -4 Pin PTH&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 4&lt;/li&gt;
&lt;li&gt;Pin pitch: 3.5mm/138mil&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Screw-Terminal-3.5mm.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-L_COPPER">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Large - Top Copper&lt;/h3&gt;
&lt;p&gt;Exposed copper logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Connector">
<description>&lt;b&gt;Pin Headers,Terminal blocks, D-Sub, Backplane, FFC/FPC, Socket</description>
<packages>
<package name="TERMBLK_254-2N">
</package>
<package name="TERMBLK_508-2N">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="K1" library="Connector" package="2X20" value="PINHD-2X20">
<attribute name="CATEGORY" value="CONNECTOR"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="PIN-HEADER"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="FLYFISH" package="SOIC8" value="EEPROM24">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="microbuilder" package="_0805MP" value="3.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="microbuilder" package="_0805MP" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="microbuilder" package="_0805MP" value="3.9k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="microbuilder" package="_0805MP" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P4" library="pinhead-2" package="1X08-S" value="MA08-1">
<attribute name="VALUE"/>
</element>
<element name="P5" library="pinhead-2" package="1X08-S" value="MA08-1">
<attribute name="VALUE"/>
</element>
<element name="P6" library="we-con" package="MA02-1" value="MA02-1"/>
<element name="P7" library="pinhead-2" package="1X08-S" value="MA08-1">
<attribute name="VALUE"/>
</element>
<element name="P8" library="pinhead-2" package="1X08-S" value="MA08-1">
<attribute name="VALUE"/>
</element>
<element name="P9" library="we-con" package="MA02-1" value="MA02-1"/>
<element name="U2" library="SparkFun-IC-Power" package="SOT23-5" value="3.3V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="VREG-12457"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="PScope" package="SO-8EP_DIO" value="AP64500SP-13">
<attribute name="BUILT_BY" value="EMA_Cory"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="https://www.diodes.com/assets/Datasheets/AP64500.pdf"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="AP64500SP-13"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="Diodes_Inc_2020-08-19"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="Diodes Inc"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="5.8A/30V/35mΩ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRANS-12988"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="PScope" package="POWERDI3333-8_UX_DIO" value="DMP3013SFV-7">
<attribute name="BUILT_BY" value="EMA_Cory"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="https://www.diodes.com/assets/Datasheets/DMP3013SFV.pdf"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="DMP3013SFV-7"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="Diodes_Inc_2020-06-18"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="Diodes Inc"/>
</element>
<element name="C2" library="microbuilder" package="_0805MP" value="100nF 100V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Diode" package="SODFL1608X70" value="BZT52C12T-7">
<attribute name="CATEGORY" value="Diode"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Zener"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="ZENER_VOLTAGE" value=""/>
</element>
<element name="C3" library="microbuilder" package="_0805MP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="microbuilder" package="_0805MP" value="12k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+12V" library="microbuilder" package="TESTPOINT_PAD_2MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="microbuilder" package="_0805MP" value="10uF 35V">
<attribute name="NAME"/>
</element>
<element name="C5" library="microbuilder" package="_0805MP" value="10uF 35V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="microbuilder" package="_0805MP" value="10uF 35V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="microbuilder" package="_0805MP" value="10uF 35V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="microbuilder" package="_0805MP" value="10uF 35V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="microbuilder" package="_0805MP" value="10uF 35V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="microbuilder" package="_0805MP" value="10uF 35V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="microbuilder" package="_0805MP" value="12k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="microbuilder" package="_0805MP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="microbuilder" package="_0805MP" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="microbuilder" package="_0805MP" value="10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="microbuilder" package="_0805MP" value="2.2k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="microbuilder" package="_0805MP" value="20k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="microbuilder" package="_0805MP" value="1.2nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="SparkFun-Coils" package="SRN6045" value="SRN6045TA-3R3Y">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="NDUC-11627"/>
<attribute name="VALUE"/>
</element>
<element name="+5V" library="microbuilder" package="TESTPOINT_PAD_2MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="microbuilder" package="_0805MP" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="microbuilder" package="TESTPOINT_PAD_2MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="microbuilder" package="_0805MP" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="microbuilder" package="_0805MP" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="microbuilder" package="_0805MP" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="Capacitor" package="CAPMP6032X280N" value="100µF 10VDC TPSC107K010T0200">
<attribute name="CATEGORY" value="Capacitor"/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value=""/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE_RATING" value=""/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="DMG2305UX">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="TRAN-14388"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="SparkFun-DiscreteSemi" package="SOT26" value="DDMT5401">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="microbuilder" package="_0805MP" value="10k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="microbuilder" package="_0805MP" value="47k 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="WP" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NO_SILK" value="JUMPER-SMT_2_NO_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="microbuilder" package="_0805MP" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="microbuilder" package="_0805MP" value="1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="EN" library="SparkFun-Jumpers" package="SMT-JUMPER_3_1-NC_PASTE_SILK" value="JUMPER-SMT_3_1-NC_PASTE_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MOT1" library="PScope" package="CONN_S4B-XH-SM4-TB_JST" value="S4B-XH-SM4-TB(LF)(SN)">
<attribute name="BUILT_BY" value="EMA_Justin"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="http://www.farnell.com/datasheets/1684882.pdf?_ga=2.23206330.1695985900.1582574926-861621671.1572890216&amp;_gac=1.58313304.1582574926.CjwKCAiAhc7yBRAdEiwAplGxX0eXyKiGfj62eRMGG7KvwS8fdWH6vWjmriwTUSfyzPNlkVLVCkx_YhoCwGcQAvD_BwE"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="S4B-XH-SM4-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="JST_2020-02-24"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="JST"/>
</element>
<element name="MOT2" library="PScope" package="CONN_S4B-XH-SM4-TB_JST" value="S4B-XH-SM4-TB(LF)(SN)">
<attribute name="BUILT_BY" value="EMA_Justin"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="DATASHEET" value="http://www.farnell.com/datasheets/1684882.pdf?_ga=2.23206330.1695985900.1582574926-861621671.1572890216&amp;_gac=1.58313304.1582574926.CjwKCAiAhc7yBRAdEiwAplGxX0eXyKiGfj62eRMGG7KvwS8fdWH6vWjmriwTUSfyzPNlkVLVCkx_YhoCwGcQAvD_BwE"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="S4B-XH-SM4-TB(LF)(SN)"/>
<attribute name="NAME"/>
<attribute name="SOURCELIBRARY" value="JST_2020-02-24"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="JST"/>
</element>
<element name="R11" library="microbuilder" package="_0805MP" value="499R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="microbuilder" package="_0805MP" value="4.99k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="Diode" package="DIOM5226X290N" value="DIODE">
<attribute name="CATEGORY" value="Diode"/>
<attribute name="DESCRIPTION" value=""/>
<attribute name="FORWARD_CURRENT" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="REVERSE_VOLTAGE" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Rectifier"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="FAN" library="PScope" package="40MM_FAN" value="40MM_FAN"/>
<element name="PWM" library="SparkFun-Jumpers" package="SMT-JUMPER_2_NO_SILK" value="JUMPER-SMT_2_NO_SILK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="INPUT" library="Connector" package="TERMBLK_508-2N" value="2828XX-2282837-2">
<attribute name="CATEGORY" value="Connector"/>
<attribute name="DESCRIPTION" value="  2 Position Wire to Board Terminal Block Horizontal with Board 5.08 mm Through Hole"/>
<attribute name="MANUFACTURER" value="TE Connectivity"/>
<attribute name="MPN" value="TC0203620000G"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMPERATURE" value="-40°C to +105°C"/>
<attribute name="PART_STATUS" value="ACTIVE"/>
<attribute name="ROHS_COMPLIANCE" value="RoHS Compliant"/>
<attribute name="SERIES" value="282837"/>
<attribute name="SUBCATEGORY" value="Terminal Block"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=" Side Wire Entry"/>
<attribute name="VALUE"/>
</element>
<element name="OLED" library="OPL_Connector" package="H4-2.54" value="4p-2.54">
<attribute name="MPN" value="P125-1104A0BS116A1"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="PScope" package="DBV6" value="TPS61165TDBVRQ1">
<attribute name="DATASHEET_URL" value="http://www.ti.com/lit/gpn/TPS61165-Q1"/>
<attribute name="DESCRIPTION" value="Automotive Catalog High Brightness White LED Driver in 2mm x 2mm QFN Package"/>
<attribute name="FAMILY_NAME" value="WHITE LED DRIVER"/>
<attribute name="GENERIC_PART_NUMBER" value="TPS61165-Q1"/>
<attribute name="INDUSTRY_STD_PKG_TYPE" value="SOT-23"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="TPS61165TDBVRQ1"/>
<attribute name="NAME"/>
<attribute name="PACKAGE_DESIGNATOR" value="DBV"/>
<attribute name="PIN_COUNT" value="6"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="Texas Instruments"/>
</element>
<element name="U6" library="SparkFun-Clocks" package="RV-3028" value="RV-3028">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-14378"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="microbuilder" package="_0805MP" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="microbuilder" package="_0805MP" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="microbuilder" package="_0805MP" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="testpad" package="B1,27" value="TPB1,27">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="19"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="Connector" package="TERMBLK_254-2N" value="2828XX-2282834-2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="microbuilder" package="_0805MP" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="microbuilder" package="_0805MP" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="Wurth_Elektronik_Passive_Capacitors_rev19a" package="8X3.5X0.9(DXAXB)" value="1F SCCR12E105SRB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="WE-NUMBER" value="870135174001/390uF"/>
</element>
<element name="D3" library="OPL_Discrete_Semiconductor" package="SOD-123" value="40V-500MA">
<attribute name="MPN" value="B0540W"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="Inductor" package="INDM3225X240" value="10µH">
<attribute name="CATEGORY" value="Inductor"/>
<attribute name="CURRENT_RATING" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value="CBC3225T100KR"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="microbuilder" package="_0805MP" value="4.7µF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="microbuilder" package="_0805MP" value="220nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="microbuilder" package="_0805MP" value="1µF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="microbuilder" package="_0805MP" value="2R / 10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="PScope" package="DBV6" value="TPS61165TDBVRQ1">
<attribute name="DATASHEET_URL" value="http://www.ti.com/lit/gpn/TPS61165-Q1"/>
<attribute name="DESCRIPTION" value="Automotive Catalog High Brightness White LED Driver in 2mm x 2mm QFN Package"/>
<attribute name="FAMILY_NAME" value="WHITE LED DRIVER"/>
<attribute name="GENERIC_PART_NUMBER" value="TPS61165-Q1"/>
<attribute name="INDUSTRY_STD_PKG_TYPE" value="SOT-23"/>
<attribute name="MANUFACTURER" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="TPS61165TDBVRQ1"/>
<attribute name="NAME"/>
<attribute name="PACKAGE_DESIGNATOR" value="DBV"/>
<attribute name="PIN_COUNT" value="6"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="Texas Instruments"/>
</element>
<element name="LED2" library="Connector" package="TERMBLK_254-2N" value="2828XX-2282834-2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="OPL_Discrete_Semiconductor" package="SOD-123" value="40V-500MA">
<attribute name="MPN" value="B0540W"/>
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="Inductor" package="INDM3225X240" value="10µH">
<attribute name="CATEGORY" value="Inductor"/>
<attribute name="CURRENT_RATING" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value="CBC3225T100KR"/>
<attribute name="NAME"/>
<attribute name="OPERATING_TEMP" value=""/>
<attribute name="PART_STATUS" value=""/>
<attribute name="ROHS_COMPLIANT" value=""/>
<attribute name="SERIES" value=""/>
<attribute name="SUB-CATEGORY" value="Fixed"/>
<attribute name="THERMALLOSS" value=""/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="microbuilder" package="_0805MP" value="4.7µF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="microbuilder" package="_0805MP" value="220nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="microbuilder" package="_0805MP" value="1µF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="microbuilder" package="_0805MP" value="2R / 10R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-4" value="">
<attribute name="PROD_ID" value="2xCONN-08399"/>
<attribute name="SF_ID" value="2xPRT-08084"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-4" value="">
<attribute name="PROD_ID" value="2xCONN-08399"/>
<attribute name="SF_ID" value="2xPRT-08084"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="microbuilder" package="_0805MP" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="microbuilder" package="_0805MP" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-L_COPPER" value="OSHW-LOGOL-COPPER"/>
</elements>
<signals>
<signal name="S$28">
</signal>
<signal name="S$33">
</signal>
<signal name="S$39">
</signal>
<signal name="S$40">
</signal>
<signal name="S$60">
</signal>
<signal name="S$61">
</signal>
<signal name="S$213">
</signal>
<signal name="S$234">
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="K1" pad="9"/>
<contactref element="K1" pad="25"/>
<contactref element="K1" pad="39"/>
<contactref element="K1" pad="6"/>
<contactref element="K1" pad="14"/>
<contactref element="K1" pad="20"/>
<contactref element="K1" pad="30"/>
<contactref element="K1" pad="34"/>
<contactref element="P5" pad="7"/>
<contactref element="P5" pad="1"/>
<contactref element="P8" pad="7"/>
<contactref element="P8" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="EPAD"/>
<contactref element="GND" pad="P$1"/>
<contactref element="C17" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="R9" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="WP" pad="1"/>
<contactref element="C20" pad="2"/>
<contactref element="EN" pad="1"/>
<contactref element="C19" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="Q1" pad="2"/>
<contactref element="INPUT" pad="1"/>
<contactref element="OLED" pad="1"/>
<contactref element="U6" pad="5"/>
<contactref element="C22" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="C26" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="U5" pad="4"/>
<contactref element="C28" pad="2"/>
<contactref element="R17" pad="1"/>
<contactref element="C29" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="U7" pad="4"/>
<contactref element="P4" pad="3"/>
<contactref element="P7" pad="3"/>
</signal>
<signal name="+3V3">
<contactref element="U1" pad="8"/>
<contactref element="R3" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="K1" pad="17"/>
<contactref element="OLED" pad="2"/>
<contactref element="U6" pad="7"/>
<contactref element="C22" pad="1"/>
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="EEPROM_SCL">
<contactref element="K1" pad="28"/>
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="EEPROM_SDA">
<contactref element="U1" pad="5"/>
<contactref element="R2" pad="1"/>
<contactref element="K1" pad="27"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="7"/>
<contactref element="R3" pad="1"/>
<contactref element="WP" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="U2" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="L1" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="+5V" pad="P$1"/>
<contactref element="U4" pad="D1"/>
<contactref element="Q2" pad="3"/>
<contactref element="C20" pad="1"/>
<contactref element="EN" pad="3"/>
<contactref element="D2" pad="1"/>
<contactref element="FAN" pad="5V"/>
</signal>
<signal name="I2C1_SDA">
<contactref element="K1" pad="3"/>
<contactref element="OLED" pad="4"/>
<contactref element="U6" pad="4"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="I2C1_SCL">
<contactref element="K1" pad="5"/>
<contactref element="OLED" pad="3"/>
<contactref element="U6" pad="3"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="GPIO4">
<contactref element="K1" pad="7"/>
</signal>
<signal name="GPIO17">
<contactref element="K1" pad="11"/>
</signal>
<signal name="GPIO27">
<contactref element="K1" pad="13"/>
</signal>
<signal name="GPIO22">
<contactref element="K1" pad="15"/>
</signal>
<signal name="SPI0_MOSI">
<contactref element="K1" pad="19"/>
<contactref element="P4" pad="7"/>
<contactref element="P7" pad="7"/>
</signal>
<signal name="SPI0_MISO">
<contactref element="K1" pad="21"/>
<contactref element="P4" pad="4"/>
<contactref element="P7" pad="4"/>
</signal>
<signal name="SPI0_SCLK">
<contactref element="K1" pad="23"/>
<contactref element="P4" pad="6"/>
<contactref element="P7" pad="6"/>
</signal>
<signal name="GPIO5">
<contactref element="K1" pad="29"/>
<contactref element="P7" pad="8"/>
<contactref element="R19" pad="1"/>
</signal>
<signal name="GPIO6">
<contactref element="K1" pad="31"/>
</signal>
<signal name="GPIO13/PWM1">
<contactref element="K1" pad="33"/>
<contactref element="R11" pad="1"/>
<contactref element="PWM" pad="2"/>
</signal>
<signal name="GPIO19">
<contactref element="K1" pad="35"/>
</signal>
<signal name="GPIO26">
<contactref element="K1" pad="37"/>
</signal>
<signal name="GPIO21">
<contactref element="K1" pad="40"/>
</signal>
<signal name="GPIO20">
<contactref element="K1" pad="38"/>
<contactref element="P6" pad="1"/>
<contactref element="P9" pad="1"/>
</signal>
<signal name="GPIO16">
<contactref element="K1" pad="36"/>
<contactref element="P6" pad="2"/>
<contactref element="P9" pad="2"/>
</signal>
<signal name="GPIO12/PWM0">
<contactref element="K1" pad="32"/>
<contactref element="U7" pad="2"/>
</signal>
<signal name="SPI0_CE1">
<contactref element="K1" pad="26"/>
<contactref element="P7" pad="5"/>
</signal>
<signal name="SPI0_CE0">
<contactref element="K1" pad="24"/>
<contactref element="P4" pad="5"/>
</signal>
<signal name="GPIO25">
<contactref element="K1" pad="22"/>
</signal>
<signal name="GPIO24">
<contactref element="K1" pad="18"/>
</signal>
<signal name="GPIO23">
<contactref element="K1" pad="16"/>
<contactref element="P4" pad="8"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="GPIO18/PWM0">
<contactref element="K1" pad="12"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="UART_RX">
<contactref element="K1" pad="10"/>
</signal>
<signal name="UART_TX">
<contactref element="K1" pad="8"/>
</signal>
<signal name="BMA1">
<contactref element="MOT1" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="P5" pad="4"/>
</signal>
<signal name="BMA2">
<contactref element="MOT1" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="P5" pad="3"/>
</signal>
<signal name="BMB2">
<contactref element="MOT1" pad="4"/>
<contactref element="J4" pad="4"/>
<contactref element="P5" pad="6"/>
</signal>
<signal name="BMB1">
<contactref element="MOT1" pad="3"/>
<contactref element="J4" pad="3"/>
<contactref element="P5" pad="5"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$4">
</signal>
<signal name="N$11">
</signal>
<signal name="N$41">
</signal>
<signal name="N$44">
</signal>
<signal name="N$45">
</signal>
<signal name="N$46">
</signal>
<signal name="N$47">
</signal>
<signal name="N$48">
</signal>
<signal name="N$49">
</signal>
<signal name="N$50">
</signal>
<signal name="N$51">
</signal>
<signal name="N$52">
</signal>
<signal name="N$53">
</signal>
<signal name="N$54">
</signal>
<signal name="N$55">
</signal>
<signal name="N$56">
</signal>
<signal name="N$57">
</signal>
<signal name="N$58">
</signal>
<signal name="N$59">
</signal>
<signal name="N$60">
</signal>
<signal name="N$61">
</signal>
<signal name="N$62">
</signal>
<signal name="N$63">
</signal>
<signal name="N$64">
</signal>
<signal name="N$65">
</signal>
<signal name="N$66">
</signal>
<signal name="N$67">
</signal>
<signal name="N$68">
</signal>
<signal name="N$69">
</signal>
<signal name="N$70">
</signal>
<signal name="N$71">
</signal>
<signal name="N$72">
</signal>
<signal name="N$73">
</signal>
<signal name="N$74">
</signal>
<signal name="N$75">
</signal>
<signal name="N$76">
</signal>
<signal name="N$77">
</signal>
<signal name="N$78">
</signal>
<signal name="N$79">
</signal>
<signal name="N$80">
</signal>
<signal name="N$81">
</signal>
<signal name="N$82">
</signal>
<signal name="N$83">
</signal>
<signal name="N$84">
</signal>
<signal name="N$85">
</signal>
<signal name="N$86">
</signal>
<signal name="N$87">
</signal>
<signal name="N$88">
</signal>
<signal name="N$89">
</signal>
<signal name="N$90">
</signal>
<signal name="N$91">
</signal>
<signal name="N$92">
</signal>
<signal name="N$93">
</signal>
<signal name="N$94">
</signal>
<signal name="N$95">
</signal>
<signal name="N$96">
</signal>
<signal name="N$97">
</signal>
<signal name="N$98">
</signal>
<signal name="N$99">
</signal>
<signal name="N$100">
</signal>
<signal name="N$101">
</signal>
<signal name="N$102">
</signal>
<signal name="N$103">
</signal>
<signal name="N$104">
</signal>
<signal name="N$105">
</signal>
<signal name="N$106">
</signal>
<signal name="N$107">
</signal>
<signal name="N$108">
</signal>
<signal name="N$109">
</signal>
<signal name="N$110">
</signal>
<signal name="N$111">
</signal>
<signal name="N$112">
</signal>
<signal name="2BMA2">
<contactref element="MOT2" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="P8" pad="3"/>
</signal>
<signal name="2BMA1">
<contactref element="MOT2" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="P8" pad="4"/>
</signal>
<signal name="2BMB1">
<contactref element="MOT2" pad="3"/>
<contactref element="J1" pad="3"/>
<contactref element="P8" pad="5"/>
</signal>
<signal name="2BMB2">
<contactref element="MOT2" pad="4"/>
<contactref element="J1" pad="4"/>
<contactref element="P8" pad="6"/>
</signal>
<signal name="VIN">
<contactref element="Q3" pad="8"/>
<contactref element="Q3" pad="7"/>
<contactref element="Q3" pad="5"/>
<contactref element="Q3" pad="6"/>
<contactref element="C2" pad="1"/>
<contactref element="Q3" pad="9"/>
<contactref element="INPUT" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="Q3" pad="4"/>
<contactref element="D1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="+12V">
<contactref element="Q3" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="D1" pad="1"/>
<contactref element="+12V" pad="P$1"/>
<contactref element="C4" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="2"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="P8" pad="8"/>
<contactref element="P5" pad="8"/>
</signal>
<signal name="FB">
<contactref element="R7" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="N$9">
<contactref element="U3" pad="1"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="C12" pad="1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="VOUT">
<contactref element="R6" pad="1"/>
<contactref element="U3" pad="8"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="U3" pad="4"/>
<contactref element="C11" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R8" pad="1"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="COMP">
<contactref element="U3" pad="6"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="U4" pad="D2"/>
<contactref element="R10" pad="2"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U4" pad="G1"/>
<contactref element="R9" pad="2"/>
<contactref element="U4" pad="S2"/>
<contactref element="U4" pad="G2"/>
</signal>
<signal name="+5V/1">
<contactref element="Q2" pad="2"/>
<contactref element="U4" pad="S1"/>
<contactref element="K1" pad="2"/>
<contactref element="K1" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="U2" pad="3"/>
<contactref element="EN" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="Q1" pad="3"/>
<contactref element="D2" pad="2"/>
<contactref element="FAN" pad="GND"/>
</signal>
<signal name="N$17">
<contactref element="R11" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="FAN" pad="PWM"/>
<contactref element="PWM" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="U2" pad="5"/>
<contactref element="C19" pad="1"/>
<contactref element="P5" pad="2"/>
<contactref element="P8" pad="2"/>
<contactref element="U5" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="L2" pad="1"/>
<contactref element="U7" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="L3" pad="1"/>
<contactref element="R18" pad="2"/>
<contactref element="R19" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U6" pad="6"/>
<contactref element="C21" pad="1"/>
<contactref element="C24" pad="1"/>
</signal>
<signal name="CLKOUT">
<contactref element="U6" pad="1"/>
<contactref element="TP4" pad="TP"/>
</signal>
<signal name="N$21">
<contactref element="U6" pad="8"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="/INT">
<contactref element="U6" pad="2"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="N$22">
<contactref element="U5" pad="5"/>
<contactref element="C25" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="U5" pad="6"/>
<contactref element="R16" pad="2"/>
<contactref element="LED1" pad="2"/>
</signal>
<signal name="N$25">
<contactref element="L2" pad="2"/>
<contactref element="U5" pad="3"/>
<contactref element="D3" pad="+"/>
</signal>
<signal name="1POS">
<contactref element="D3" pad="-"/>
<contactref element="LED1" pad="1"/>
<contactref element="C26" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="U7" pad="5"/>
<contactref element="C28" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="U7" pad="6"/>
<contactref element="R17" pad="2"/>
<contactref element="LED2" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="L3" pad="2"/>
<contactref element="U7" pad="3"/>
<contactref element="D4" pad="+"/>
</signal>
<signal name="2POS">
<contactref element="D4" pad="-"/>
<contactref element="LED2" pad="1"/>
<contactref element="C29" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
